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	MODEL
	SP-30048
	SP-300512
	Configurable

	

	· MAIN INFO	

	Rated Voltage
	48V
	51.2V
	

	Rated Capacity
	300Ah
	

	Battery Power
	13.44kWh
	15.36kWh
	

	Battery Type
	LFP
	

	[bookmark: _GoBack]Cycling Lifespan
	>6000 Cycles
	

	Max.Parallel Capacity
	15 units
	√


	· CHARGE&DISCHARGE

	Max.Charging Voltage
	54V
	57.6V
	√

	Dischare Cut-off Voltage
	40.5V
	44.8V
	√

	Max.Charging Current
	205A
	√

	Peak Charging Current
	210(1S)
	√

	Max.Discharging Current
	205
	√

	Peak Discharging Current
	210(1S)
	√

	
	
	

	· GENERAL

	Net Weight
	115kg
	120kg
	

	Gross Weight
	135kg
	140kg
	

	Product Size(L×W×H)
	700×500×270MM
	

	Package Size(L×W×H)
	980×640×465MM
	

	Communication
	RS485/RS232/CAN/Wifi/Bluetooth
	√

	Storage Condition
	6months@25℃ 
3months@35℃ 
1month@45℃
	

	Charging Temp.Range
	0℃ to 65℃（32°F to 149°F)
	

	Discharging Temp.Range
	-10℃ to 65℃（314°F to 149°F)
	

	Cooling Method
	Passive Cooling
	

	
	
	

	· STANDARD

	Transportation
	UN38.3/MSDS/TDG
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